#!/bin/ash

PATH=/usr/sbin:/usr/bin:/sbin:/bin

# Default to the udev device manager
USE_UDEV_NORMAL=1

# Insert ctrl character
# ctrl-V then esc will print ^[
# ctrl-V then ctrl-shift-m will print ^M
BACK_UP="\033[1K\033[0G"
NORMAL="\033[0m"
WARN="\033[33;1m"
BAD="\033[31;1m"
BOLD="\033[1m"
GOOD="\033[32;1m"


# From KNOPPIX LINUXRC
# Reset fb color mode
RESET="]R"
# ANSI COLORS
# Erase to end of line
CRE="
[K"
# Clear and reset Screen
CLEAR="c"
# Normal color
NORMAL="[0;39m"
# RED: Failure or error message
RED="[1;31m"
# GREEN: Success message
GREEN="[1;32m"
# YELLOW: Descriptions
YELLOW="[1;33m"
# BLUE: System mesages
BLUE="[1;34m"
# MAGENTA: Found devices or drivers
MAGENTA="[1;35m"
# CYAN: Questions
CYAN="[1;36m"
# BOLD WHITE: Hint
WHITE="[1;37m"

# Clear screen with colormode reset
# echo "$CLEAR$RESET"
# echo "$CLEAR"
# Just go to the top of the screen
# echo -n "[H[J"

KV="`uname -r`"
KMAJOR=`echo $KV | cut -f1 -d.`
KMINOR=`echo $KV | cut -f2 -d.`
KVER="${KMAJOR}.${KMINOR}"
MISCOPTS='idebug detect'

if [ "${KMAJOR}" -eq 2 -a "${KMINOR}" -ge '6' ]
then
	KV_2_6_OR_GREATER="yes"
fi

QUIET=1
ROOT_LINKS='bin sbin lib lib32 lib64 boot usr opt'
ROOT_TREES='etc root home var'
INSMOD='insmod'
if [ "${KMINOR}" -gt '4' ]
then
	KSUFF='.ko'
else
	KSUFF='.o'
fi

REAL_ROOT=''
CDROOT=0
CDROOT_DEV=''
NEW_ROOT="/newroot"
CONSOLE="/dev/console"

# Only sections that are in by default or those that
# are not module groups need to be defined here...
HWOPTS='usb firewire keymap cache evms2 sata lvm2 dmraid bladecenter'
MY_HWOPTS='usb firewire sata dmraid'
